**How to setup range extender mode via management page**

Product line: Wireless Model number: A300/A301


We can set range extender mode for A300 to extend our wireless network via button or management page based on web. This article will guide you set range extender mode via UI. Before setting A300, please make sure that you can get internet if you connect your computer to upper router directly. Steps are as follow：

**Part 1**: [Login its homepage](#OLE_LINK7)


**Part 2**: [Configure extender function](#OLE_LINK3)




**1** Launch a browser and usually it will login automatically. If not，input **192.168.0.254** or **re.tendacn.com** in the address bar and press Enter.



1. Enter the default password **admin** and click **OK**.




1. Then the following page will appear.






**1** Click **Wizard,** select **Range Extender Mode** and click **Next**




**2** Click **Open Scan**, select the remote router's wireless network (SSID), say Tenda\_881218, click **OK**.


and close Scan.



1. Enter the remote device’s security key and click **Save**;



**4** In the appearing dialogue box click **OK**;



**5** Click **System Status** to check the bridge status. When the bridge status displays **Connected**, bridged successfully.

