**How to setup Tenda D152 PPPoE mode**

Product line: ADSL Model number: D152

This article will guide you how to setup Tenda D152 PPPoE mode and the steps as below.

**Note**: If you have no idea about what is the internet connection type, the accounts (user name and password) please call your ISP for them.

**Part 1**: Connect the devices

**Part 2**: Configure your computer

**Part 3**: Setup the router

**Part 4**: Check whether you can access internet



Connect the broadband line with the **LAN/WAN** port of D152, and then connect your computer with **IPTV** port of D152 by a cable.



**Note:** after connection the **SYS** light should be blinking, the **WLAN** light should be on or blinking, the **LAN/WAN, IPTV** light should be on or blinking.



1 Click on **Network Connection Icon** on the system bar, then click on **Open Network and Sharing Center**.



2 Click on **Change adapter settings**.



3 **Right** click on **Local Area Connection**, then choose the **Properties** option.



4 **Double** click on **Internet Protocol Version 4(TCP/IPv4)4.** 

5 Choose **Obtain an IP address automatically** and **Obtain DNS server address automatically** and then click **OK**.



6 Also click on **OK** on the first **Local Connection Properties** window.





**3.1 Setup the router in home page**

3.1.1 Open a browser then type **192.168.1.1** in the **Address bar**, click on **Enter**.



3.1.2 Type the **Username** and **Password** as **admin** in the bars then click on **Login** to login the setting page of the router.



3.1.3 Setup D152 in home page ,choose **ETH**, **PPPoE** and then please type in **user name** and **password** (you can consult your ISP for it if you don’t know). You can also change the **SSID** and **wireless key**, and then click **OK**.



3.1.4 Click on **Advanced** on the right of the page to login the advanced setting page.



3.1.5 Click on **Management** and **Reboot** then hit on the **Reboot** button to reboot the router for refreshing the device info.



3.1.6 After reboot, Click on **Device Info, WAN,** then check the **WAN** Status if the Connection **Status** shows **Connected** that means you can access internet, please check.



 **If you can’t, please click** [**h****e****re**](#OLE_LINK9) **and follow the steps below.**

**3.2 Setup the router in advanced settings page**

3.2.1 Click on **Management** and **Settings, Restore Default** then hit on the **Restore Default Settings** button.



3.2.2 Click on **Advanced Setup**, **Layer2 Interface**, **ETH Interface** and **Add**. And keep the default setting, click **Apply/Save**. Then you can see ETH WAN Interface exists. 



3.2.3 Click **WAN Service** and **Add**, keep the eth1/eth1 and click **Next**, then choose **PPP over Ethernet** **(PPPoE)** and click **Next**, please type in **user name** and **password** (you can consult your ISP for it if you don’t know).Click **Next** and click **Apply/Save**.















3.2.4 Click on **Management** and **Reboot** then hit on the **Reboot** button to reboot the router for refreshing the device info.





1 Click on **Advanced** to login the advanced setting page, then check the **WAN** Status if the Connection **Status** shows **Connected** that means you can access internet, please check.

