**How to setup the router for 3G/4G Router** **mode**

Product line: 3G/4G Model number: 4G302

There are four internet connection modes for the router. This article will guide you how to setup the router for 3G/4G Router mode and the steps as below.

**Part 1**: Connect the devices

**Part 2**: [Login to the home page](#_Hlk371926727" \s "4,29,53,0,,Configure your computer)

**Part 3**: [Setup the router](#OLE_LINK5)

**Part 4**: [Check whether you can access internet](#_Hlk371926892" \s "4,89,126,0,,Check whether you can access int)



Connect the RJ-45 port of the router with an Ethernet cable. The topology is as below:





**1** Open a browser then type **192.168.0.1** in the **Address bar**, click **Enter**. Type the **Password**（default: admin ）in the bars then click on the **Login** button to login the setting page.

**Note**: if you cannot login the management page, please click HERE.





**1** click the **wizard** option, then choose **3G/4G Router Mode**, click on **next.**



**2** Choose **country, service provider**, then type in the **APN** and other information if you have. Then click **next**.

Note: if you don’t know the Service Provider, please choose **Auto**.



**3** Change the SSID, channel, security mode, WPA/WPA2 Cipher and Key, click **next**.



**4** Click **Finish**, then the router will reboot automatically.





Type the Password as **admin** login to the homepage, then Click on **Status-running status** to check on if **Internet Connection** **Status** shows **Connected**, that means you can access internet, please check.

