**How to setup the router for Dynamic IP internet connection mode**

Product line: Wireless Model number: F1200

There are three internet connection modes for the router. This article will guide you how to setup the router for Dynamic IP mode and the steps as below.

**Note**: if you have no idea about the internet connection type and the accounts please call your ISP for then.

**Part 1**: Connect the devices


**Part 2**: [Configure your computer](#_Hlk371926727" \s "4,29,53,0,,Configure your computer)

**Part 3**: [Setup the router](#OLE_LINK5)

**Part 4**: [Check whether you can access internet](#_Hlk371926892" \s "4,89,126,0,,Check whether you can access int)




Connect the modem with the **WAN** port of the router, then connect your computer with one of the **LAN** ports of the router by a cable.




**Note**: after connection the **SYS** light should be blinking, the **WLAN** light should be on or blinking, the **WAN** light should be on or blinking.




**1** Click on **Network Connection Icon** on the system bar, then click on **Open Network and Sharing Center**. (Here is for windows 7, other operating system please click [HERE](http://www.tendacn.com/tendacn/Support/show.aspx?articleid=2263).)

****


**2** Click on **Change adapter settings**.

****


**3 Right** click on **Local Area Connection**, then choose **Properties** option.

****


**4 Double** click on **Internet Protocol Version 4(TCP/IPv4)**

****

**5** Choose **Obtain an IP address automatically** and **Obtain DNS server address automatically** and then click **OK**.

****

**6** Also click on **OK** on the first **Local Connection Properties** window

****




**1** Open a browser then type **192.168.0.1** in the **Address bar**, click **Enter**.

C:\Users\Jane Lee\Desktop\N301做FAQ\browser.PNG

**Note**: if you cannot login the management page, please click HERE.

**2** Type the **Password**（default: admin ）in the bars then click on the **Login** button to login the setting page.



**3** Choose the **Dynamic IP** option, then set a **2.4G Security** for the wireless security , then click on **Save** to save the settings, then click on **Advanced**.

DHCP.tif

Note: the **2.4G Security** should be at least **8** characters.

**4** Click on **Tools**, click on **Reboot**, and then press the **Reboot** button to reboot the router for refreshing the device info.

reboot.tif



Type the User Name and Password as admin to login the setting page the click on **Advanced** to login the advanced setting page, and then check on **Status** if the **WAN** **Status** shows **Connected** that means you can access internet, please check.

DHCP status.tif