**How to setup the router for PPPOE internet connection mode**

Model number: FH303

There are three internet connection modes for the router. This article will guide you how to setup the router for PPPOE mode and the steps are as below.

**Note**: if you have no idea about the internet connection type and the accounts please call your ISP for help.

**Part 1**: [Connect the device](#OLE_LINK1)

**Part 2**: [Configure your computer](#_Hlk371926727" \s "4,29,53,0,,Configure your computer)

**Part 3**: [Setup the router](#OLE_LINK5)

**Part 4**: [Check whether you can access internet](#_Hlk371926892" \s "4,89,126,0,,Check whether you can access int)



Connect the modem with the **WAN** port of the router, and then connect your computer with one of the **LAN** ports of the router by a cable.



Note: After connection the **SYS** light should be blinking, the **WLAN** light should be on or blinking, the **WAN** light should be on or blinking.



**1** Click **Network Connection Icon** on the system tray, then click **Open Network and Sharing Center**. (Here is for windows 7, other operating system please click [HERE](http://www.tendacn.com/tendacn/Support/show.aspx?articleid=2263).)

**Icon.tif**

**2** Click on **Change adapter settings**.

**Change.tif**

**3 Right** click **Local Area Connection**, then choose **Properties** option.

**local.tif**

**4 Double** click on **Internet Protocol Version 4(TCP/IPv4)**

**IPV4.tif**

**5** Choose **Obtain an IP address automatically** and **Obtain DNS server address automatically** and then click **OK**.

**IP.tif**

**6** Also click **OK** on the first **Local Connection Properties** window

**ok1.tif**


****

**1** Open a browser then type **192.168.0.1** in address bar, click **Enter**.


browser.tif

**Note**: if you cannot login the home page, please click [HERE](http://www.tendacn.com/tendacn/Support/show.aspx?articleid=2087).

**2** Fill in admin in the **Password** field, click **OK** to login.




**3** Choose the **PPPOE** option, then type the **ISP Username** and **ISP Password** in the correct bars, then set a **2.4G** **Security** as you want, click **OK** to save the settings, then click **Advanced** to login the advanced setting page.



**Note**: the **Security** **Key** should be at least **8** characters.

**4** Click on **Tools**, then click on **Reboot**, and then press the **Reboot The Router** button to reboot the router for refreshing the device info.





Type the User Name and Password as admin then Click on **Advanced** to login the advances setting page, and then check on the **Status** if the **Connection** **Status** shows **Connected** that means you can access internet, please check.

