**How to setup the router for Static IP internet connection mode?**

Product line: Wireless Model number: N301

There are five internet connection modes for the router. This article will guide you how to setup the router for Static IP mode and the steps as below.

**Part 1**:[Connect the devices](#_Hlk371927967" \s "4,0,19,0,,Connect the devices)


**Part 2**:[Configure your computer](#_Hlk371928006" \s "4,30,53,0,,Configure your computer)

**Part 3**:[Setup the router](#_Hlk371928037" \s "4,63,79,0,,Setup the router)

**Part 4**:[Check whether you can access internet](#_Hlk371928076" \s "4,89,126,0,,Check whether you can access int)



Connect the modem with the **WAN** port of the router, then connect your computer with one of the **LAN** ports by a cable.




Attention: After connection the **SYS** light should be blinking, the **WLAN** light should be on or blinking, the **WAN** light should be on or blinking.




Open the **Network and Sharing Center**.(Here is for win7, other computer please click [HERE](http://www.tendacn.com/tendacn/Support/show.aspx?articleid=2263).)


**1** Click on **Network Connection Icon** on the system bar, then click on **Open Network and Sharing Center**.

****


**2** Click on **Change adapter settings**.

****


**3 Right** click on **Local Area Connection**, then choose the **Properties** option.

****


**4 Double** click on **Internet Protocol Version 4(TCP/IPv4)**

****

**5** Choose **Obtain an IP** and **DNS server address automatically** and then click **OK**.

****

**6** Also click on **OK** on the first **Local Connection Properties** window.

****

****

**1**Open a browser then type 192.168.0.1 in the **Address bars**, click **Enter**.

C:\Users\Jane Lee\Desktop\N301做FAQ\browser.PNG

NOTE: If you cannot login the management page, please click [HERE](http://www.tendacn.com/tendacn/Support/show.aspx?articleid=2087).


**2**Clickon **Advanced** in the middle of the page.

home.tif

**3**Click on the **Internet Connection Setup**, open the **Dropdown Menu** of the **Internet Connection Type** then choose the **Static IP** option, after that type the **accounts** that provided by your ISP then click on **OK** to save the settings.

static IP.tif

**4** After setting, please click on **Tools**, click on **Reboot** then hit the **Reboot The Router** button to reboot the router for refreshing the device info.





**1** Click **Advanced**, then check the **Status** if the **Connection Status** shows **Connected** that means you can access internet, please check.

