**How to change the SSID and wireless password?**

 Model number: N301

The cause of the change SSID and wireless password is to protect the wireless network. This article will guide you how to change the SSID and wireless password.

**Part 1**:[Login the homepage of the router](#_Hlk372193340" \s "4,49,82,0,,Login the homepage of the router)

**Part 2**:[Change the SSID and wireless password](#_Hlk372193369" \s "4,8,46,0,,Change the SSID and wireless pas)

**Part 3**:[Reboot the router](#_Hlk372193406" \s "4,93,110,0,,Reboot the router)



Open a browser then type 192.168.0.1 in the **Address bar**, click **Enter**.



**Note**: If you cannot login the management page, please click [HERE](http://www.tendacn.com/tendacn/Support/show.aspx?articleid=2087).



**1** Click on **Advanced** on the home page.



**2**Click on**Wireless**, then click on **Wireless Basic Settings** and making sure that check the **Wireless** function. Then you can change the **Primary SSID** as you want. Then open the drop down menu of **Network Mode** and choose the mode as **11b/g/n mixed mode**. Let the other settings as defaulted, then click on **OK** to save the settings.



**3** Click on **Wireless Security**, **Disable** the WPS settings then open the dropdown menu of the **Security Mode** and choose the mode as **WPA-PSK (recommended)** and **AES** as the **WPA Algorithms**, then change the **Security Key** as you want and click **OK** to save the settings.



**Note**: Security Key must be between 8-63 ASCII characters.



Click on **Tools**, then hit on the **Reboot The Router** button to refresh the device info.



Now you can use your laptop to search the new SSID and enter the new password to connect to it.

**Note**:

If you do not how to connect your Wi-Fi please click [HERE](http://www.tenda.cn/tendacn/Support/show.aspx?articleid=2262).