**How to set wireless mode for this router**

Product line: Mobile Broadband Model number: 4G600/4G630

There are 3 working modes. This article will guide you how to set 4G600/4G630 as wireless router mode.

**Note**: Before setting 4G600/4G630, please make sure that you can access to internet when cable from modem is connected to computer directly.

Steps are as follow.

**Part 1**: [Connect the devices](#OLE_LINK11)


**Part 2**: [Configure your computer](#OLE_LINK10)

**Part 3**: [Setup the router](#OLE_LINK4)

**Part 4**: [Check whether you can access internet](#OLE_LINK3)



Connect the cable form modem with the **WAN** port of the router, then connect your computer with one of the **LAN** ports of the router by a cable.



**Note**: after connection the **SYS** light should be blinking, the **WiFi** light should be on or blinking, the **WAN** light should be on or blinking.



**1** Click on **Network Connection Icon** on the system bar, then click on **Open Network and Sharing Center**. (Here is for windows 7, other operating system please click [HERE](http://www.tendacn.com/tendacn/Support/show.aspx?articleid=2263).)

****

**2** Click on **Change adapter settings**.

****

**3 Right** click on **Local Area Connection**, then choose **Properties** option.

****

**4 Double** click on **Internet Protocol Version 4(TCP/IPv4)**

****

**5** Choose **Obtain an IP address automatically** and **Obtain DNS server address automatically** and then click **OK**.

****

**6** Also click on **OK** on the first **Local Connection Properties** window

****


****

**1** Open a browser then type **192.168.0.1** in the **Address bar**, click **Enter**.


C:\Users\Jane Lee\Desktop\N301做FAQ\browser.PNG

**Note**: if you cannot login the management page, please click [HERE](http://www.tendacn.com/tendacn/Support/show.aspx?articleid=2087).


**2** Type the **Password** in the bars then click on the **Login** button to login the setting page.




1. Choose the **Wireless Router Mode** option, then click on **Next**.




1. Choose the correct internet connection type, if you are not sure which to select please ask your ISP for help.



1. Configure your wireless network: **SSID**, **Channel**, **Key** and then click **Next**.



**6** Click **Finish** and wait for the device to restart.





Type the Password as admin to login the setting page then click on **Status** to check the connection status of 4G600.If it shows connected then you can enjoy your internet.

